{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Foglio1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Foglio1","index":0,"n_rows":26,"n_cols":4,"rows_kept":26,"cut":false,"hidden":false,"merged":[]}
["Model name",{"$f":"NFmodel()","v":"RCcolumnSection"}]
[]
["b",0.4,"m"]
["h",0.3,"m"]
[]
["Rebar no.",16]
["Rebar cover",0.04,"m"]
["Rebar diam.",1.2E-2,"m"]
[]
["N",-120,"kN","(minus sign for compression)"]
["Myy",40,"kNm"]
["Mzz",55,"kNm"]
[]
["RESULTS"]
["Mry",55.398251744430198]
["Mrz",76.172435354541193]
["Nmin",708.08766592215397]
["Nmax",-2408.0877588060498]
["Curvature",2.2603310867556601E-2]
["ds",0.42117929273213101]
["AsTens",1.13097335529233E-3]
["AsCompr",6.7858401317539804E-4]
["yn",0.15484457212963801]
["Yangle",159.479875529775]
["UsageRatio",0.72204544307191398]
["errCode",0]